**

**MASTER**

**Medtronic Enlite Post-Test**

1) During sensor insertion, after I click and release the green button, I immediately click the button a second time and pull up on the serter

( ) Yes

**( ) No**

2) To remove needle housing I must stabilize the sensor with one hand and pull straight up on the plastic safety housing from the top, after which I must deposit it in a sharps container

**( ) Yes**

( ) No

3) The green charge light on the minilink transmitter, indicating a charge (which lasts up to 7 days when fully charged), should light (check all that apply):

**( ) After being removed from the blue charger, just momentarily**

( ) After being removed from the charger, and continue to remain lit until charge is depleted

**( ) After being attached to the sensor, just momentarily**

( ) After being attached to the sensor, and continue to remain lit until charge is depleted